(footprint "PowerPAIR_3x3S_BWL"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(tags "SiZ250DT")
	(property "Reference" "REF**"
		(at 0 -6 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "b6484d24-eede-4808-b862-569627955741")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "PowerPAIR_3x3S_BWL"
		(at 0.25 1.45 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "4129ef8c-85fe-443f-9f6b-1ebb4fffb84e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "PowerPAIR_3x3S_BWL"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "bd320f5f-3612-402a-8c3c-624681667577")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://www.vishay.com/docs/77227/siz250dt.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "af0546ec-b5b9-48f1-9060-0d7a40e276de")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Land Pattern for PowerPAIR ® 3 x 3S BWL"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c047d57d-079d-4605-8e49-e22926241f31")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(zone_connect 2)
	(attr smd)
	(fp_line
		(start -1.778 -1.3335)
		(end -1.778 -1.7145)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "c1347e54-2c61-4367-ae4e-5da7cffbd906")
	)
	(fp_line
		(start -1.778 1.3335)
		(end -1.778 1.7145)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "0d355805-b8f6-4637-92c8-ffedf78348eb")
	)
	(fp_line
		(start -1.778 1.7145)
		(end -1.397 1.7145)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "006f547e-4d9f-4641-92bc-01e8900a56e3")
	)
	(fp_line
		(start 1.397 1.7145)
		(end 1.778 1.7145)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "a45b7717-4fe9-4078-a43b-24f963e59c40")
	)
	(fp_line
		(start 1.778 -1.7145)
		(end 1.397 -1.7145)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "56532f5f-c0a8-4496-9b27-14e3da32f020")
	)
	(fp_line
		(start 1.778 -1.3335)
		(end 1.778 -1.7145)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "ce442c1b-dd1e-4c7b-ad53-c83862083272")
	)
	(fp_line
		(start 1.778 1.3335)
		(end 1.778 1.7145)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "374bfd4a-d43c-4bee-af5d-440655b8cae5")
	)
	(fp_line
		(start -2 -1.8)
		(end 2 -1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "38c08409-70ea-48ff-8c4c-cad4e53171b1")
	)
	(fp_line
		(start -2 1.8)
		(end -2 -1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "e3d43786-f184-413c-9185-2eb52ac6b920")
	)
	(fp_line
		(start 2 -1.8)
		(end 2 1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "7ac81297-d9f6-45c2-9284-f22910132eda")
	)
	(fp_line
		(start 2 1.8)
		(end -2 1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "2d2435e3-233a-420f-87e2-b8d4f3e0a041")
	)
	(fp_rect
		(start -1.65 -1.65)
		(end 1.65 1.65)
		(stroke
			(width 0.01)
			(type default)
		)
		(fill none)
		(layer "User.1")
		(uuid "4642dd27-1ffa-48b6-90e9-bccef7c59f23")
	)
	(fp_text user "${REFERENCE}"
		(at 0.25 2.95 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "5f730847-6651-4d54-9dcf-f58df9a33033")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -1.65 -0.315)
		(size 0.62 0.44)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "2c0fd9e2-c238-4977-9473-12c95a3a8f97")
	)
	(pad "1" smd rect
		(at -1.65 0.315)
		(size 0.62 0.44)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "be73a822-1754-4956-bfcb-5c13b2ab12be")
	)
	(pad "1" smd rect
		(at -1.65 0.975)
		(size 0.62 0.44)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "44774e99-4412-4ae1-bff5-551bc3894003")
	)
	(pad "1" smd rect
		(at -0.6625 0.025)
		(size 0.935 2.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_paste_margin -0.12)
		(thermal_bridge_angle 45)
		(uuid "2c905ec6-2b12-49b4-ba2d-19cf55450c53")
	)
	(pad "2" smd rect
		(at 0.5575 0)
		(size 1.005 2.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_paste_margin -0.12)
		(thermal_bridge_angle 45)
		(uuid "10c02127-ed8b-4993-92d3-5a13747939a2")
	)
	(pad "3" smd rect
		(at 1.65 -0.315)
		(size 0.62 0.44)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "a94f6c59-106c-4ac3-9f09-6dd1c27eb9f5")
	)
	(pad "3" smd rect
		(at 1.65 0.315)
		(size 0.62 0.44)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "3da0b1b7-58ce-4576-87bc-02a3ee01c81a")
	)
	(pad "3" smd rect
		(at 1.65 0.975)
		(size 0.62 0.44)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "73198135-7950-4aa4-8659-cd3e5bd3f48f")
	)
	(pad "4" smd rect
		(at 1.65 -0.975)
		(size 0.62 0.44)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "40a9cf16-1f0b-449a-a443-6c573d1ede7d")
	)
	(pad "5" smd rect
		(at -1.65 -0.975)
		(size 0.62 0.44)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "c2fc0da1-0401-400c-a986-00411e1ec5ab")
	)
	(model "${KIPRJMOD}/libs/DUALMOSFETS/SIZ250DT-T1-GE3.stp"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
