(footprint "ESP32-S3-WROOM-1" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "ESP32-S3-WROOM-1 is a powerful, generic Wi-Fi + Bluetooth LE MCU modules that have Dual core CPU , a rich set of peripherals, provides acceleration for neural network computing and signal processing workloads. They are an ideal choice for a wide variety of application scenarios related to AI + Internet of Things (AIoT), such as wake word detection and speech commands recognition , face detection and recognition, smart home, smart appliance, smart control panel, smart speaker etc.")
  (tags "esp32-s3")
  (attr smd)
  (fp_text reference "REF**" (at 0 -17.05) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6a494ce2-3e36-47fb-b812-2b7bd4826e62)
  )
  (fp_text value "ESP32-S3-WROOM-1" (at 0 12) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 783caf9d-4324-476e-a13f-fdc754e21b09)
  )
  (fp_text user "Antenna Area" (at 0 -12.75) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6e73b5a0-8e83-4e1d-ab2d-f2e051dcd480)
  )
  (fp_text user "Antenna Area" (at 0 -12.75) (layer "Eco2.User")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 177f12b8-8bd0-4a12-ab65-379074d27aa7)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d1bd5684-5703-4f21-8944-f8b5e664753a)
  )
  (fp_line (start -9 -15.75) (end -9 -9)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f09cb53d-3c7f-41e1-9378-7a694a6c7669))
  (fp_line (start -9 -15.75) (end 9 -15.75)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 634c074d-f53a-4f17-a01c-c427dd463e8b))
  (fp_line (start -9 9) (end -9 9.75)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1da9e0f4-67f1-4c87-b759-aa83e451c712))
  (fp_line (start -9 9.75) (end -8 9.75)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9ee2fba6-6fe2-4858-a44e-be5b98019ec5))
  (fp_line (start 9 -15.75) (end 9 -9)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp eb034fbd-6e78-4af0-bae0-69aac2ddde9d))
  (fp_line (start 9 -9.81) (end -9 -9.81)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8eb6d55e-a524-4dfa-9f3c-f6e2b6c699d3))
  (fp_line (start 9 9) (end 9 9.75)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b6834186-afee-4ae0-9a93-925c0bb9e7de))
  (fp_line (start 9 9.75) (end 8 9.75)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d9dd9499-26b8-4e11-910f-0111dd31ef04))
  (fp_line (start -9 -15.75) (end 9 -15.75)
    (stroke (width 0.12) (type solid)) (layer "Eco2.User") (tstamp 7d0b72d7-5116-4177-9258-1878f8bef9cc))
  (fp_line (start -9 -9.81) (end 9 -9.81)
    (stroke (width 0.12) (type solid)) (layer "Eco2.User") (tstamp 8abdc6f3-9a5f-4da3-9c34-b23c59c8590c))
  (fp_line (start -9 9.75) (end -9 -15.75)
    (stroke (width 0.12) (type solid)) (layer "Eco2.User") (tstamp 0ca656fa-48af-4a1c-a601-053be9ebbad1))
  (fp_line (start 9 -15.75) (end 9 9.75)
    (stroke (width 0.12) (type solid)) (layer "Eco2.User") (tstamp 84e68fa2-bb13-4777-9070-15cd537d0952))
  (fp_line (start 9 9.75) (end -9 9.75)
    (stroke (width 0.12) (type solid)) (layer "Eco2.User") (tstamp b7478048-2075-4121-afa4-bb285dd4be82))
  (fp_line (start -10.5 -16.05) (end -10.5 11)
    (stroke (width 0.12) (type solid)) (layer "F.CrtYd") (tstamp 2c8b8865-c8e2-4a82-94a6-ef91b67d531b))
  (fp_line (start -10.5 11) (end 10.5 11)
    (stroke (width 0.12) (type solid)) (layer "F.CrtYd") (tstamp 80d0bbc2-14f7-448d-8aa6-8c3905d3d9e6))
  (fp_line (start 10.5 -16.05) (end -10.5 -16.05)
    (stroke (width 0.12) (type solid)) (layer "F.CrtYd") (tstamp 25835b1c-7754-4fc7-b535-341b92f55e01))
  (fp_line (start 10.5 -16.05) (end 10.5 11)
    (stroke (width 0.12) (type solid)) (layer "F.CrtYd") (tstamp 1c186107-50c1-4782-abbf-69f5ab7ac836))
  (pad "1" smd rect (at -9 -8.3) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 50487783-7a00-479f-b02e-a22f2e69705c))
  (pad "2" smd rect (at -9 -6.97) (size 2 0.86) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 74edfefe-235e-4cba-b7c7-0b3ef3f4e3d8))
  (pad "3" smd rect (at -9 -5.72) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp f06e6b01-b7fe-465d-a080-7a947f0af6d0))
  (pad "4" smd rect (at -9 -4.45) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp b3f3b826-ad37-4009-a80e-3d8374cc0c38))
  (pad "5" smd rect (at -9 -3.18) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 9131a2a0-95c6-4580-b1cf-f88f8563575e))
  (pad "6" smd rect (at -9 -1.91) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp cda21c99-c83e-4d0b-8571-0ed3b4b0e679))
  (pad "7" smd rect (at -9 -0.64) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 6cbd0f57-25f9-4b44-8052-5c8529f27482))
  (pad "8" smd rect (at -9 0.63) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 7bfde213-a42f-4eef-a297-a0e64894c965))
  (pad "9" smd rect (at -9 1.9) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 277311bb-ff9f-4a6e-9cb5-34a5d0e9cdfa))
  (pad "10" smd rect (at -9 3.17) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp ef54d737-e14c-4d0c-a88b-0b55885d2cf7))
  (pad "11" smd rect (at -9 4.44) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp f9825c58-09cb-46e1-96b1-d7fd60161d40))
  (pad "12" smd rect (at -9 5.71) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 80ead716-583c-4503-93ec-8d1c5a6014a1))
  (pad "13" smd rect (at -9 6.98) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp cd959b9f-9c4c-436a-979c-f6aeaafb6760))
  (pad "14" smd rect (at -9 8.25) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 48a365e1-9db9-40b7-9444-7fc8ebac0bcd))
  (pad "15" smd rect (at -6.985 9.625 90) (size 1.75 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 3a8d36b7-ae2b-4099-920c-31906ad65e30))
  (pad "16" smd rect (at -5.715 9.625 90) (size 1.75 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 30173bb5-e9ac-4359-a3eb-f7d5adce1e87))
  (pad "17" smd rect (at -4.445 9.625 90) (size 1.75 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp f8334445-03d8-4bd9-86b6-6d3e42f0464a))
  (pad "18" smd rect (at -3.175 9.625 90) (size 1.75 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 09230549-fedb-477a-acf3-e3278c038d0d))
  (pad "19" smd rect (at -1.905 9.625 90) (size 1.75 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 55ffd2ad-bf08-48f9-804e-e09166a85009))
  (pad "20" smd rect (at -0.635 9.625 90) (size 1.75 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 116ed370-6f22-4c44-a0c5-65c8afcd76af))
  (pad "21" smd rect (at 0.635 9.625 90) (size 1.75 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 62656f08-78ab-42c1-9b0e-309545d0a6fa))
  (pad "22" smd rect (at 1.905 9.625 90) (size 1.75 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 8485f993-1e88-41ed-9182-3d4a971f99e0))
  (pad "23" smd rect (at 3.175 9.625 90) (size 1.75 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 92896f5e-a071-4348-a09f-24d20ffc5258))
  (pad "24" smd rect (at 4.445 9.625 90) (size 1.75 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 1c22fd53-5eba-4b4e-8fd4-bd0eb10aaa50))
  (pad "25" smd rect (at 5.715 9.625 90) (size 1.75 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp fd7db19c-179f-420c-83c1-251bf5ec82d0))
  (pad "26" smd rect (at 6.985 9.625 90) (size 1.75 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 8e04eaa5-b8a3-42b4-91bf-117771bca3c0))
  (pad "27" smd rect (at 9 8.25 180) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 2a5fdc24-53cd-4dcf-904b-b1f9b160516e))
  (pad "28" smd rect (at 9 6.98 180) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 00e44920-5998-4350-aeb4-9640bdd7172e))
  (pad "29" smd rect (at 9 5.71 180) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 45eb453f-e0ae-4db3-9c1d-e15003abe653))
  (pad "30" smd rect (at 9 4.44 180) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 72b57dd8-1622-4a76-8600-8cfe0daf5e9b))
  (pad "31" smd rect (at 9 3.17 180) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp a7bfb3d7-0315-4e87-9b1e-57b0d2c0efda))
  (pad "32" smd rect (at 9 1.9 180) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp d3e0c4f7-434f-48fe-87b3-e2c61acd4905))
  (pad "33" smd rect (at 9 0.63 180) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp c3f7ab00-389b-4625-aacc-888299416a0a))
  (pad "34" smd rect (at 9 -0.64 180) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 47be7051-02f5-4711-b225-3a4f00922cb4))
  (pad "35" smd rect (at 9 -1.91 180) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp ad9c8ceb-b0ce-44d3-b2dc-d0d049b15f81))
  (pad "36" smd rect (at 9 -3.18 180) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 6534dc4e-1b20-4fa0-bf2a-be27e43b11d0))
  (pad "37" smd rect (at 9 -4.45 180) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 3770d143-f149-483c-8a17-3b2681e7d7be))
  (pad "38" smd rect (at 9 -5.72 180) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 8798b91f-06df-4395-bce5-dcd7a16e347b))
  (pad "39" smd rect (at 9 -6.99 180) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp e9365a3d-136f-4dee-ad48-b9b90adfb53f))
  (pad "40" smd rect (at 9 -8.26 180) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 29771e24-4118-4caa-bbbc-d0798b82d7fc))
  (pad "41" smd rect (at -2.9 -1.94 180) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 232b6e8e-d710-4438-8fb1-240292206ac9))
  (pad "41" smd rect (at -2.9 -0.54 180) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 137e64e5-e8c2-4d69-bb13-98f6c722f3b7))
  (pad "41" smd rect (at -2.9 0.86 180) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp dff2af33-d35f-431f-9740-20d62ac876b9))
  (pad "41" smd rect (at -2.9 0.86 180) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp dff2af33-d35f-431f-9740-20d62ac876b9))
  (pad "41" smd rect (at -1.5 -1.94 180) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp b692b8a2-428c-424f-b34e-d76890b7a7f8))
  (pad "41" smd rect (at -1.5 -1.94 180) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp b692b8a2-428c-424f-b34e-d76890b7a7f8))
  (pad "41" smd rect (at -1.5 -0.54 180) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 0ba22266-1a20-4193-ad95-5e3f6d1a1299))
  (pad "41" smd rect (at -1.5 0.86 180) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 50d810a4-964f-4e7a-abcb-544ef87fc914))
  (pad "41" smd rect (at -0.1 -1.94 180) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 325964ac-707a-4db9-9457-88ae8b311329))
  (pad "41" smd rect (at -0.1 -0.54 180) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 8d57aefc-46be-46ca-9783-caa0625b0b06))
  (pad "41" smd rect (at -0.1 0.86 180) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp af66518f-af54-48c0-b506-27977596c4f8))
  (zone (net 0) (net_name "") (layers "*.Cu") (tstamp 34781a2f-5beb-4476-8bb4-599ba67b983b) (name "antenna keepout") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints not_allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 9 -9.8)
        (xy -9 -9.8)
        (xy -9 -15.75)
        (xy 9 -15.75)
      )
    )
  )
  (model "${KICAD7_3RD_PARTY}/3dmodels/com_github_espressif_kicad-libraries/espressif.3dshapes/ESP32-S3-WROOM-1.STEP"
    (opacity 0.7500)    (offset (xyz -9 -9.75 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
