
(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "DRV8313PWP" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -12.7 31.48 0.0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Value" "DRV8313PWP" (id 1) (at -12.7 -33.02 0.0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Footprint" "DRV8313PWP:SOP65P640X120-29N" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "RS_Components_1457432_Purchase_URL" "https://www.snapeda.com/api/url_track_click/https%253A//uk.rs-online.com/web/p/motor-driver-ics/1457432//%253Futm_campaign%253Dbuynow%2526utm_medium%253Daggregator%2526utm_source%253Dsnapeda%2526cm_mmc%253Daff-_-uk-_-snapeda-_-1457432/?unipart_id=287728&manufacturer=Texas Instruments&part_name=DRV8313PWP&search_term=drv8313" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MF" "Texas Instruments" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "SNAPEDA_PACKAGE_ID" "102627" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Package" "HTSSOP-28 Texas Instruments" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "RS_Components_8136469P_Purchase_URL" "https://www.snapeda.com/api/url_track_click/https%253A//uk.rs-online.com/web/p/motor-driver-ics/8136469p//%253Futm_campaign%253Dbuynow%2526utm_medium%253Daggregator%2526utm_source%253Dsnapeda%2526cm_mmc%253Daff-_-uk-_-snapeda-_-8136469P/?unipart_id=287728&manufacturer=Texas Instruments&part_name=DRV8313PWP&search_term=drv8313" (id 8) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Check_prices" "https://www.snapeda.com/parts/DRV8313PWP/Texas+Instruments/view-part/?ref=eda" (id 9) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "STANDARD" "Manufacturer Recommendations" (id 10) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "PARTREV" "D" (id 11) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/DRV8313PWP/Texas+Instruments/view-part/?ref=snap" (id 12) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MP" "DRV8313PWP" (id 13) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=287728&manufacturer=Texas Instruments&part_name=DRV8313PWP&search_term=drv8313" (id 14) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Description" "\n65-V max, 3-A peak 3-phase motor driver\n" (id 15) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "RS_Components_8136469_Purchase_URL" "https://www.snapeda.com/api/url_track_click/https%253A//uk.rs-online.com/web/p/motor-driver-ics/8136469//%253Futm_campaign%253Dbuynow%2526utm_medium%253Daggregator%2526utm_source%253Dsnapeda%2526cm_mmc%253Daff-_-uk-_-snapeda-_-8136469/?unipart_id=287728&manufacturer=Texas Instruments&part_name=DRV8313PWP&search_term=drv8313" (id 16) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MANUFACTURER" "Texas Instruments" (id 17) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MAXIMUM_PACKAGE_HEIGHT" "1.2 mm" (id 18) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (symbol "DRV8313PWP_0_0"
      (rectangle (start -12.7 -30.48) (end 12.7 30.48)
        (stroke (width 0.254)) (fill (type background))
      )
      (pin input line (at -17.78 -7.62 0) (length 5.08)
        (name "COMPN"
          (effects (font (size 1.016 1.016)))
        )
        (number "13"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -17.78 -10.16 0) (length 5.08)
        (name "COMPP"
          (effects (font (size 1.016 1.016)))
        )
        (number "12"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -17.78 12.7 0) (length 5.08)
        (name "EN1"
          (effects (font (size 1.016 1.016)))
        )
        (number "26"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -17.78 10.16 0) (length 5.08)
        (name "EN2"
          (effects (font (size 1.016 1.016)))
        )
        (number "24"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -17.78 7.62 0) (length 5.08)
        (name "EN3"
          (effects (font (size 1.016 1.016)))
        )
        (number "22"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -17.78 2.54 0) (length 5.08)
        (name "IN1"
          (effects (font (size 1.016 1.016)))
        )
        (number "27"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -17.78 0.0 0) (length 5.08)
        (name "IN2"
          (effects (font (size 1.016 1.016)))
        )
        (number "25"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -17.78 -2.54 0) (length 5.08)
        (name "IN3"
          (effects (font (size 1.016 1.016)))
        )
        (number "23"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -17.78 20.32 0) (length 5.08)
        (name "~{RESET}"
          (effects (font (size 1.016 1.016)))
        )
        (number "16"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -17.78 17.78 0) (length 5.08)
        (name "~{SLEEP}"
          (effects (font (size 1.016 1.016)))
        )
        (number "17"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 17.78 0.0 180.0) (length 5.08)
        (name "~{FAULT}"
          (effects (font (size 1.016 1.016)))
        )
        (number "18"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 17.78 180.0) (length 5.08)
        (name "CPL"
          (effects (font (size 1.016 1.016)))
        )
        (number "1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 15.24 180.0) (length 5.08)
        (name "CPH"
          (effects (font (size 1.016 1.016)))
        )
        (number "2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 27.94 180.0) (length 5.08)
        (name "VCP"
          (effects (font (size 1.016 1.016)))
        )
        (number "3"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 22.86 180.0) (length 5.08)
        (name "VM"
          (effects (font (size 1.016 1.016)))
        )
        (number "4"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 22.86 180.0) (length 5.08)
        (name "VM"
          (effects (font (size 1.016 1.016)))
        )
        (number "11"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 25.4 180.0) (length 5.08)
        (name "V3P3"
          (effects (font (size 1.016 1.016)))
        )
        (number "15"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -15.24 180.0) (length 5.08)
        (name "EXP"
          (effects (font (size 1.016 1.016)))
        )
        (number "29"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 17.78 10.16 180.0) (length 5.08)
        (name "OUT1"
          (effects (font (size 1.016 1.016)))
        )
        (number "5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 17.78 7.62 180.0) (length 5.08)
        (name "OUT2"
          (effects (font (size 1.016 1.016)))
        )
        (number "8"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 17.78 5.08 180.0) (length 5.08)
        (name "OUT3"
          (effects (font (size 1.016 1.016)))
        )
        (number "9"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -20.32 180.0) (length 5.08)
        (name "PGND1"
          (effects (font (size 1.016 1.016)))
        )
        (number "6"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -22.86 180.0) (length 5.08)
        (name "PGND2"
          (effects (font (size 1.016 1.016)))
        )
        (number "7"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -25.4 180.0) (length 5.08)
        (name "PGND3"
          (effects (font (size 1.016 1.016)))
        )
        (number "10"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -27.94 180.0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "14"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -27.94 180.0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "20"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -27.94 180.0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "28"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin no_connect line (at -17.78 -15.24 0) (length 5.08)
        (name "NC"
          (effects (font (size 1.016 1.016)))
        )
        (number "21"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 17.78 -7.62 180.0) (length 5.08)
        (name "~{COMPO}"
          (effects (font (size 1.016 1.016)))
        )
        (number "19"
          (effects (font (size 1.016 1.016)))
        )
      )
    )
  )
)