(footprint "L_Bourns-SRU1028_10.0x10.0mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Bourns SRU1028 series SMD inductor, https://www.bourns.com/docs/Product-Datasheets/SRU1028.pdf")
	(tags "Bourns SRU1028 SMD inductor")
	(property "Reference" "L2"
		(at 0 0 0)
		(layer "F.SilkS")
		(uuid "1a9f76b5-0a16-4397-96f8-fa98dd06ae5f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "27uH"
		(at 0 6.2 0)
		(layer "F.Fab")
		(uuid "d13a7b35-33ce-44fc-871a-64affaccd35b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Inductor_SMD:L_Bourns-SRU1028_10.0x10.0mm"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d842c679-fcdd-4eae-9a43-961d1d81e1eb")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "414b3c2b-7e28-4aa0-819d-835067e49004")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Inductor"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b025a729-acd4-4e46-a48d-b3adf2a6057a")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Mouser" " 652-SRU1038-270Y"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "60c986e2-1cdc-49db-a5d9-00f639e55077")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.8 -5.2)
		(end -5 -2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "234c7fc9-d87b-40e1-9e4d-55c7b2359b2a")
	)
	(fp_line
		(start -1.8 -5.2)
		(end 1.8 -5.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7179246f-e006-47bc-8ca6-98dc57221985")
	)
	(fp_line
		(start -1.8 5.2)
		(end -5 2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c7b942bf-8bed-4a43-8d36-14e379f593b4")
	)
	(fp_line
		(start 1.8 -5.2)
		(end 5 -2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6c092c13-3ded-46c6-8421-150bfdd077e2")
	)
	(fp_line
		(start 1.8 5.2)
		(end -1.8 5.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a9d276f9-009b-40e2-a53e-d033522c25ce")
	)
	(fp_line
		(start 1.8 5.2)
		(end 5 2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2abed6f0-c705-499b-a822-5ea438acfd85")
	)
	(fp_line
		(start -5.65 -2)
		(end -5.65 0)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "07bf2777-c939-4aaa-994e-574d309db3ff")
	)
	(fp_line
		(start -5.65 -2)
		(end -5.65 0)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "6af5858d-2e12-40d0-ba12-b614b0b9ba65")
	)
	(fp_line
		(start -5.65 2)
		(end -5.65 0)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "7c8681bf-20e9-4c0a-8747-e026efc76cf3")
	)
	(fp_line
		(start -2.4 -5.334)
		(end -5.65 -2)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b3ecb243-3bbe-4e49-9e00-31fc145dffd6")
	)
	(fp_line
		(start -2.4 5.334)
		(end -5.65 2)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "9af31c52-8f69-4d0f-89a9-25327ed05cf4")
	)
	(fp_line
		(start 2.4 -5.334)
		(end -2.4 -5.334)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f61f4c3c-0bb6-4214-bb52-bf90c3141ca0")
	)
	(fp_line
		(start 2.4 -5.334)
		(end 5.65 -2)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "96b9eca0-b835-4c59-ae6f-1cd82014f67b")
	)
	(fp_line
		(start 2.4 5.334)
		(end -2.4 5.334)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "d8953c7d-a879-44ea-8821-c7561178e00c")
	)
	(fp_line
		(start 2.4 5.334)
		(end 5.65 2)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "3a69e58b-c600-4a16-b1ed-31bd82ec899b")
	)
	(fp_line
		(start 5.65 -2)
		(end 5.65 0)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f9ef39fb-d7e1-4372-86b1-0b265d202c1b")
	)
	(fp_line
		(start 5.65 2)
		(end 5.65 0)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "63e50097-72a5-4a1f-9e26-0e2704d796f1")
	)
	(fp_line
		(start -5 -1.7)
		(end -1.7 -5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1042b9f8-2326-4e41-afe3-635318114422")
	)
	(fp_line
		(start -5 1.7)
		(end -5 -1.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5814a2d4-cf7a-4f58-a548-6227a20fd71e")
	)
	(fp_line
		(start -1.7 -5)
		(end 1.7 -5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f2522e5b-445b-419b-8a82-5c459f7bc4d2")
	)
	(fp_line
		(start -1.7 5)
		(end -5 1.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3fa7fadc-5e1d-498d-8efe-7e05a44189a1")
	)
	(fp_line
		(start 1.7 -5)
		(end 5 -1.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "63b1f7ab-c415-4c4f-a077-3e1d4cdc9804")
	)
	(fp_line
		(start 1.7 5)
		(end -1.7 5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ef7326c1-dfeb-4f06-851d-1dd7b5f6fcfb")
	)
	(fp_line
		(start 5 -1.7)
		(end 5 1.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "edfae774-2b5d-4cf8-b97e-9e0fc12c887c")
	)
	(fp_line
		(start 5 1.7)
		(end 1.7 5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2ce02fd4-acaa-448e-add2-710f16399016")
	)
	(fp_circle
		(center 0 0)
		(end 3.7 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "31969423-b453-4e8b-9c3a-5db1e8318b70")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "173ec9da-6869-4796-b81b-2dbf4cb6bab7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -4.5 0)
		(size 1.8 3.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "5045eee8-6f73-464f-afd3-051aeec5f479")
	)
	(pad "2" smd rect
		(at 4.5 0)
		(size 1.8 3.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "a2bf1f92-9813-4332-b75c-2ae601be4c3e")
	)
	(model "${KIPRJMOD}/libs/SRU1038-270Y.stp"
		(offset
			(xyz 0 0 0.05)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 180 0)
		)
	)
)
